Broadwind Energy/Safe Compressor (2 units available)

* Year built 2015
* 250 HP Electric Drive @ 1185 RPM
* 480 volts three phase @ 60 hz
* 3 throw 4 stage
* 44 PSIG Suction
* 4500 PSIG Max Delivery pressure
* 536 SCFM @ 44 PSIG
* Priority panel installed
	+ High, Med, Low bank storage
	+ Direct Fill
	+ Requires remote storage

Some spare parts available

1 unit needs HMI communication reprogramed to PLC (replaced HMI)

Both units were mechanically good at last use (~6 months)